These are ingredients to make bio diesel fuel:

It is made by taking vegetable oil and mixing it with an alcohol eg. methanol, and a catalyst, usually potassium hydroxide [cuastic soda] at a temperature of 140F or 55 deg C to cause a chain reaction known as transerification, whereby the free fatty acids are made into esters.

We will be using these same ingredients for our Bio feces fuel (BFF).

But we will be adding human feces and other ingredients for yet figured out which other chemicals will be put in.